# GENERAL DESCRIPTION

* 1. The unit shall be a highly vandal-resistant steel card reader surface mount, model ETP-SMCR, no substitutions. The surface mount shall house an ADA-compliant communication device manufactured by Talk-A-Phone Co. and shall include a non-metallic mounting plate for mounting of a card reader or a similar external device.

# CONSTRUCTION

* 1. The unit shall be constructed of a 14-gauge steel with a multi-coat, rust-inhibitive coating to withstand prolonged exposure to harsh environments and weigh approximately 35 lbs.
	2. The unit shall measure 25" W x 6.76" D x 14" H.
	3. An opening shall be cut in the unit, measuring 6.75" W x 10" H, to accommodate mounting of any Talk-A-Phone 400-Series or 500-Series emergency phone (e.g. VOIP-500K).
	4. The unit shall include three stackable acrylic adapters, each measuring 12" W x 12" H x 0.5” thick to provide magnetic isolation for a card reader. The adapters shall have a 2" diameter wire opening surrounded by four pre-drilled holes.
	5. The unit shall include two 1.125" diameter conduit entries: one on the bottom and one on the rear of the unit.
	6. The unit shall include a hinged panel for easy installation of a phone and a card reader.
	7. The unit shall be painted safety yellow (standard), with a variety of customs colors available.

# MOUNTING

* 1. The Surface Mount shall have four 0.34" holes on the back wall for surface mounting on a wall or strapping to a pole.
	2. Unit shall be compatible with Talk-A-Phone models ETP-GP-C Car Height Gooseneck Pedestal, ETP-GP-T Truck Height Gooseneck Pedestal and ETP-GP-D Dual Height Gooseneck Pedestal.
	3. Pole Mounting Kit, model ETP-PMKT, shall be available for strapping to a pole.

# OPTIONS

* 1. Finish
		1. Surface Mount Accessory shall be available painted in custom colors and with custom lettering.
	2. Communications
		1. Surface Mount Accessory shall accept any Talk-A-Phone 400-series or 500-series flush mounting emergency phone.

# WARRANTY

* 1. Surface Mount Accessory shall be warrantied against any defects in material and workmanship, under normal use, for a period of two years from date of installation. In the event system is found by manufacturer to be defective within the warranty period, manufacturer shall repair and/or replace any defective parts, provided the equipment is returned to manufacturer.

# MANUFACTURER

* 1. The Manufacturer shall be Talk-A-Phone Co. (773) 539-1100, 7530 N. Natchez Ave, Niles, Illinois 60714-3804, www.talkaphone.com. THERE ARE NO EQUIVALENTS.