VERSION: 1.0.2.7

RELEASE DATE: 08/09/2016

BUG FIXES:

1. Audio issue fixed for call paths having a Media Gateway.
2. Expanded UDP buffer to support interoperability with Avaya Aura phone system.
3. Enhanced audio and added DTMF recovery logics for correct detection of the transmitted DTMF digits.
4. SMTP mail client fixed. The "Email Notification Profile" feature which distributes email notifications on such events as SIP deregistration, call activation, and physical link restore now works successfully.
5. Condition where the phone fails to register if only two servers are configured for registration under the ‘SIP Settings’ page is fixed.
6. Fixed the issue with default values not correctly set by (a) factory reset and (b) WEB-GUI-> Maintenance-> Reset to Default.
7. Extended minSE support to allow values up to 86,400 seconds on the SIP Registrar. Previously the highest allowed value was 1800 seconds.
8. Forced the system to reboot if the IP assignment scheme is changed from Static to DHCP to ensure correct initialization of the DHCP client.

NEW FEATURES AND ENHANCEMENTS:

1. Implemented support as a direct IP speaker on the InformaCast server.
2. Implemented support for TCPDUMP for easy collection of IP traffic from the device itself.
3. Implemented a mechanism to download all the files required for troubleshooting from the device GUI itself.
4. Implemented support for external ringer notification through the Auxiliary Outputs.
5. Implemented new GUI scheme and Talkaphone colors.
6. Expanded support for IE 11 and Firefox 42.

KNOWN ISSUES:

(1) The "HTTP" option for a firmware upgrade fails to execute properly. It is recommended that the "HTTP" firmware upgrade option be avoided.

----------------------------------------------------------------