# GENERAL DESCRIPTION

* 1. The unit shall be a highly vandal-resistant stainless steel emergency phone Surface Mount Accessory with Door, model ETP-SMB, no substitutions, suitable for mounting on an outdoor wall or pole. The Surface Mount shall house an ADA-compliant communication device manufactured by Talk-A-Phone Co.
  2. The communication device shall be capable of activating optional peripheral devices (i.e. activating a preset on a PTZ dome camera).

# Construction

* 1. The unit shall be constructed of #4 vertical brushed marine grade (316) stainless steel and weigh approximately 11 lbs.
  2. The unit shall integrate an easy to use, push-button release to open the door that complies with ADA-guidelines on latch-opening devices.
  3. The unit shall measure 10.93" W x 15.93" H x 7.01" D.
  4. The unit shall be designed such that a 400-Series or a 500-Series flush mounting Emergency Phone with handset shall mount inside enclosure with door closed.
  5. Unit shall have a 7/8" conduit entry hole on bottom.

# MOUNTING

* 1. The Surface Mount shall have four 0.25" x 0.5” slots on two mounting flanges for surface mounting on a wall and two 0.35” holes for strapping unit to a pole.
  2. Pole Mounting Kit, model ETP-PMKT, shall be available for strapping to a pole.

# Options

* 1. Finish
     1. Surface Mount Accessory shall be available painted in custom colors and with custom lettering.
  2. Communications
     1. Surface Mount Accessory shall accept any Talkaphone 400-series or 500-series flush mounting emergency phone.
  3. Magnetic Door Switch
     1. Enclosure shall be available with a magnetic two-pole switch that activates when door is open as model ETP-SMB-MS.

# Compliance

* 1. Enclosure shall be certified to UL Standard 60950.
  2. Enclosure shall be NEMA 4X compliant (conduit hole must be sealed with rated equipment).

# Warranty

* 1. Equipment shall be warrantied against any defects in material and workmanship, under normal use, for a period of twenty-four months from date of installation. In the event system is found by manufacturer to be defective within the warranty period, manufacturer shall repair and/or replace any defective parts, provided the equipment is returned to manufacturer.

# MANUFACTURER

* 1. The Manufacturer shall be Talk-A-Phone Co. (773) 539-1100, 7530 N. Natchez Ave, Niles, Illinois 60714-3804, www.talkaphone.com. THERE ARE NO EQUIVALENTS.

**NOTE: Due to a policy of continuous improvement, Talk-A-Phone Co. reserves the right to change specifications and appearance without notice.**